|  |  |
| --- | --- |
| COUNTY | ITEM NO. |
|       |       |
| PROJECT NO. | FEDERAL NUMBER | PROJECT |
|       |       |       |
| PARCEL(S) |       |
| **[ ]**  | Improvements and items to be removed have been discussed. |
| **[ ]**  | The successful bidder has been given a set of plans for all parcels on this contract. |
| **[ ]**  | The successful bidder must obtain a Kentucky Overweight/Overdimension Permit Worksheet (TC 95-10) from the Kentucky Transportation Cabinet, Division of Motor Carriers before moving an improvement on or across any highway or structure maintained by the Kentucky Transportation Cabinet. |
| **[ ]**  | **Kentucky 811 – Before You Dig (BUD)**Discussed the requirements of the contractor to contact Kentucky 811 before work can begin in accordance with guidelines set forth by the Kentucky Public Service Commission and outlined in KRS 367.4901 to 367.4917 and provide BUD Confirmation Number(s).BUD Confirmation Number(s)  |
| **[ ]**  | **Specification for Removal of Improvements – Disposal of Materials** Discussed the requirements for disposal of materials and the need to provide applicable disposal receipts upon completion of the project. |
| **[ ]**  | **Specification for Removal of Improvements – Recovery of Refrigerant**Discussed the requirements for recovery of refrigerants and need to provide receipt for recovery upon completion of project. |
| **[ ]**  | **Specification for Removal of Improvements – Open Burning**No open burning of improvements, trash, debris or waste material will be permitted on this contract. Discussed steps to take should open burning by unknown parties take place. |
| **[ ]**  | **Specification for Removal of Improvements – Clearance Procedures*** Cesspools, septic tanks and similar installations are to be pumped by a licensed septic tank service prior to removal / demolition. Must provide paid receipt from the service that performed the pumping.
* Basements shall be cleared of all debris, appliances, partition wall, wooden floors, and other items. Concrete basement floors, basement walls and foundation walls shall be completely removed.
* Water and monitoring wells are not to be filled but must be temporarily covered.
 |
| **[ ]**  | The following items have been discussed:      |
| We, the undersigned, do hereby verify that the successful bidder was provided the information indicated. |
|  |  |  |  |
| Successful Bidder | Date | Property Management Agent | Date |