SPECIAL NOTE FOR JOINT SEALING

**1. DESCRIPTION.** Perform all work in accordance with the Kentucky Transportation Cabinet, Department of Highway’s Standard Specifications for Road and Bridge Construction and applicable Supplemental Specifications, the Standard Drawings, (current editions), this Note and Attached Detailed Drawings. Section references are to the Standard Specifications. This work consists of the following: (1) Furnish all labor, materials, tools, and equipment, (2) Saw Cut New Overlay, (3) Install Sealant as specified and (4) Any other work specified as part of this contract.

**2. MATERIALS.**

**A. Silicone Rubber Sealants.**

See Section 807.03.05.

**3. CONSTRUCTION.**

**A. Saw Cut New Overlay (Deck).**

Saw cut new over as indicated in the attached detailed drawings.

**B. Remove Existing Sealant (Sidewalk and Mountable Median).**

Remove existing sealant as indicated in the attached detailed drawings.

**B. Installing Silicone Rubber Sealants.**

Furnish and install the Silicone Rubber Sealing in accordance with 807.03.05.

after saw cutting the new overlay and removing the existing sealant.

**C.** **Verifying Field Conditions.** The Contractor shall field verify all joint locations and manufactures before ordering any material. New material that is unsuitable due to variation in existing structure shall be replaced at the Contractors expense.

**4. MEASUREMENT.**

**A. JOINT SEALING.** The Department will measure the quantity in linear feet from inside face of parapet to inside face of parparat along the centerline of the joint.

**5. PAYMENT.**

**A. JOINT SEALING (08540) -** Payment at the contract unit price per linear foot is full compensation for saw cutting removing existing sealant, furnishing, and installing the new sealant and all incidental items necessary to complete the work within the specified pay limits as specified by this note and the standard specification.