SPECIAL NOTE FOR JOINT SEAL REPLACEMENT

**1. DESCRIPTION.** Perform all work in accordance with the Kentucky Transportation Cabinet, Department of Highway’s Standard Specifications for Road and Bridge Construction and applicable Supplemental Specifications, the Standard Drawings, (current editions), this Note and Attached Detailed Drawings. Section references are to the Standard Specifications. This work consists of the following: (1) Furnish all labor, materials, tools, and equipment, (2) Remove existing joint seal, (3) Install joint seal as specified and (4) Any other work specified as part of this contract.

**2. MATERIALS.**

**A. Expansion Joint Seals.**

See The Division of Material’s list of approved materials for preformed compression joint seal designs.

**3. CONSTRUCTION.**

**A. Remove Existing Materials.**

Remove the existing seal. Armored edges to remain.

**B. New Joint Material.** Use a system listed in 2. Materials to reseal joints. Install as recommended from the manufacture and in accordance with Section 609.03.04. Provide the engineer with the manufacture’s documents for installation.

**C.** **Verifying Field Conditions.** The Contractor shall field verify all joint openings, locations, and manufacture before ordering any material. New material that is unsuitable due to variation in existing structure shall be replaced at the Contractors expense.

**4. MEASUREMENT.**

**A. JOINT SEAL REPLACEMENT.** The Department will measure the quantity in linear feet from gutter line to gutter line along the centerline of the joint. The Department will not measure the portion of the new seal extending through the barrier. The portion of the joint seal extending through the barriers will be considered incidental.

**5. PAYMENT.**

**A. JOINT SEAL REPLACEMENT (23386EC) -** Payment at the contract unit price per linear foot is full compensation for removing specified existing materials, furnishing, and installing the new specified system, and all incidental items necessary to complete the work within the specified pay limits as specified by this note and the standard specification.