**SPECIAL NOTE FOR FILL REPAIR**

**1. DESCRIPTION.** Perform all work in accordance with the Kentucky Transportation Cabinet, Department of Highway’s Standard Specifications for Road and Bridge Construction and applicable Supplemental Specifications, the Standard Drawings (Current Editions), this Note, and the attached detail drawings. Section references are to the Standard Specifications. This work consists of the following: (1) Furnish all labor, materials, tools, and equipment, (2) Place all flowable fill and all cyclopean stone rip rap and (3) Any other work specified as part of this contract.

**2. MATERIALS.**

**A. Flowable Fill.** See Section 601.

**B. Cyclopean Stone Rip Rap.** See Section 703.

**3. CONSTRUCTION.**

**A. Placing Flowable Fill.** Place flowable as shown in the attached detailed drawings and in accordance with Section 601.

**B.** **Placing Cyclopean Stone Rip Rap.** Place cyclopean stone rip rap as shown in the attached detailed drawing and in accordance with Section 607.

**5. MEASUREMENT.**

1. **Flowable Fill.** The Department will measure the quantity inCubic Yards

**B. Cyclopean Stone Rip Rap**. The Department will measure the quantity in Tons.

**6. PAYMENT.**

**A. Flowable Fill (02220).** Payment at the contract unit price per Cubic Yard is full compensation for placing all flowable fill and all incidental items necessary to complete the work within the specified pay limits as specified by this note and as shown on the attached detailed drawings.

**B. Cyclopean Stone Rip Rap (08019).** Payment at the contract unit price per Ton is full compensation for placing all cyclopean stone rip rap and all incidental items necessary to complete the work within the specified pay limits as specified by this note and as shown on the attached detailed drawings.