Special Note for Striping on High Friction Surface treatments

1. **Description**

Installation of pavement striping, temporary, durable waterborne markings, and/or thermoplastic markings on High Friction Surface (HFS) Treatments.

1. **Construction**

Conduct striping under lane closures meeting the conditions of the MUTCD and Kentucky Standard Drawings and Specifications, current editions. Upon initial completion of the HFS installation, install temporary striping as the Engineer directs. Upon completion of the 48-hour vacuum sweeping, install either durable waterborne markings or thermoplastic markings, whichever the Contract specifies or as directed by the Engineer. Temporary Pavement Striping will comply with all applicable requirements within Section 112. Thermoplastic markings shall comply with all applicable requirements within Section 714. Durable waterborne markings shall comply with all applicable requirements within Section 713.

1. **Measurement**

The Department will measure striping quantities in linear feet. NOTE: On HFS installations, the Contractor is advised that it may be necessary to install multiple passes of striping in order to achieve the required specifications. Final payment will be based on the actual length of the final striping regardless of the number passes required to meet specifications.

1. **PAYMENT**

The Department will make payment for the completed and accepted quantities under the following:

Code Pay Item Pay Unit

 ---- Pavement Striping - Temporary Linear Foot

 ---- Durable Waterborne Marking, width, color Linear Foot

 ---- Pavement Striping - Thermoplastic, width, color Linear Foot

The Department will consider payment as full compensation for all work required under this note, Section 112, Section 713, and Section 714.