**Special Note for Signage**

All sign sheeting shall be from the Cabinet’s List of Approved Materials.

All permanent signs and sign components shall be fabricated using Type XI sheeting.

The following signs and sign components shall be fabricated using Type XI fluorescent yellow sheeting:

* + Horizontal Alignment Signs and Plaques, including signs shown in Figure 2C-1 of the MUTCD
	+ All Advisory Speed (W13-1P) plaques

The following signs shall be fabricated using Type XI fluorescent yellow-green sheeting:

* School and school bus warning signs, including the fluorescent yellow-green signs shown in Figures 7B-1 and 7B-6 of the MUTCD and other school-related warning signs that are not included in the MUTCD.
* Bicycle Warning (W11-1) signs and SHARE THE ROAD (W16-1P) plaques or diagonal downward pointing arrow (W16-7P) plaques that supplement Bicycle Warning signs.
* Pedestrian Warning signs and diagonal downward pointing arrow plaques that supplement Pedestrian Warning signs.
* In-Street Pedestrian Crossing (R1-6) signs and Overhead pedestrian Crossing (R1-9) signs
* Supplemental plaques to any of the previously listed signs