
BRIDGE DETAIL FOR PAVING PROJECT

**BRIDGE NUMBER**

****

**DIMENSIONS** **ELEVATION**

W= W = bridge width curb to curb

T = T = thickness of existing bituminous overlay

L1 =

L1 & L2 = length of approach pavement to be removed

L2 =

TR = TR = thickness to be removed and replaced on bridge

L = L = length of bridge

PR = PR = thickness to be removed and replaced on pavement

Note: The Engineer will determine lengths L1 & L2  by using a transition rate of 100 ft/inch of thickness.

1-98330 Bridge Detail Single Bridge  
01/02/2012