**INITIAL TREATMENT**

Construct parabolic pavement crown from centerline on 1/4":1' slope as directed by the Engineer.