**JPC PAVEMENT THICKNESS**

Contrary to Sections 501.03.21, 501.05.01, 502.03, and 502.05, the Department will accept JPC Pavement and JPC Pavement 24/48/72 pavement thickness according to *Special note for Acceptance of JPC Pavement Thickness* [*10T*].