|  |
| --- |
| *Utility coordination efforts conducted by the project sponsor have determined that no significant utility relocation work is required to complete the project. Any work pertaining to these utility facilities is defined in the bid package and is to be carried out as instructed by the Kentucky Transportation Cabinet. The contractor will be responsible for any coordination or adjustments that are discussed or quantified in the proposal.*  **THE FOLLOWING RAIL COMPANIES HAVE FACILITIES IN CONJUNCTION WITH THIS PROJECT AS NOTED**  **No Rail Involved  Minimal Rail Involved (See Below)  Rail Involved (See Below)** |
| |  | | --- | | **UNDERGROUND FACILITY DAMAGE PROTECTION – BEFORE YOU DIG**  The contractor shall make every effort to protect underground facilities from damage as prescribed in the Underground Facility Damage Protection Act of 1994, Kentucky Revised Statute KRS 367.4901 to 367.4917.  It is the contractor’s responsibility to determine and take steps necessary to be in compliance with federal and state damage prevention directives.  The contractor is instructed to contact KY 811 for the location of existing underground utilities.  Contact shall be made a minimum of two (2) and no more than ten (10) business days prior to excavation.  The contractor shall submit Excavation Locate Requests to the Kentucky Contact Center (KY 811) via web ticket entry.  The submission of this request does not relieve the contractor from the responsibility of contacting non-member facility owners, whom are to be contacted through their individual Protection Notification Center.  It may be necessary for the contractor to contact the County Court Clerk to determine what utility companies have facilities in the area.  Non-compliance with these directives can result in the enforcement of penalties.  **SPECIAL CAUTION NOTE – PROTECTION OF UTILITIES** | | The contractor will be responsible for contacting all utility facility owners on the subject project to coordinate his activities.  The contractor will coordinate his activities to minimize and, where possible, avoid conflicts with utility facilities. Due to the nature of the work proposed, it is unlikely to conflict with the existing utilities beyond minor facility adjustments. Where conflicts with utility facilities are unavoidable, the contractor will coordinate any necessary relocation work with the facility owner and Resident Engineer.  The  Kentucky Transportation Cabinet maintains the right to remove or alter portions of this contract if a utility conflict occurs. | | The utility facilities as noted in the previous section(s) have been determined using data garnered by varied means and with varying degrees of accuracy: from the facility owners, a result of S.U.E., field inspections, and/or reviews of record drawings. The facilities defined may not be inclusive of all utilities in the project scope and are not Level A quality, unless specified as such.  It is the contractor’s responsibility to verify all utilities and their respective locations before excavating. | | ***Please Note: The information presented in this Utility Note is informational in nature and the information contained herein is not guaranteed.*** | |
|  |

**AREA UTILITIES CONTACT LIST AS PROVIDED BY KY 811**

Utility Company/Agency Contact Name Contact Information