**Special Note for Tubular Markers – Pexco City Post (Embedded Anchor Cup)**

1. **DESCRIPTION**

Except as provided herein, perform all work in accordance with the Department's Standard Specifications, interim Supplemental Specifications, Standard and Sepia Drawings, and Special Notes and Special Provisions, current editions. Article references are to the Standard Specifications. This project shall consist of furnishing all labor, equipment, materials, and incidentals for the following:

(1) Maintaining and Controlling Traffic; (2) Installing Pexco City Post (Embedded Anchor Cup); and (3) All other work specified in the Contract.

1. **MATERIALS**

All materials shall be sampled and tested in accordance with the Department's Sampling Manual and the materials shall be available for sampling a sufficient time in advance of the use of the materials to allow for the necessary time for testing unless otherwise specified in these Notes.

1. **Maintain and Control Traffic.** See Traffic Control Plan.
2. **Tubular Markers.** Furnish Pexco City Post Embedded Anchor Cup Tubular Marker which includes delineator posts/panels, adhesive shield, rubber gasket, and anchor cup. The complete system shall be compliant with NCHRP 350 or MASH. Manufacturer’s documentation validating this compliance shall be provided to the Engineer prior to installation.System color shall match the adjacent pavement marking color. The upright delineator posts shall be 28 inches in height and 3 inches in diameter. The upright delineator posts are to be uniformly spaced according the Detail Sheets found elsewhere in the Proposal. Post color shall match the adjacent pavement marking color. Each post shall have a “double wrap” of retroreflective sheeting of color matching the post and adjacent pavement marking. Upright posts should be easily replaceable under traffic conditions and shall be fabricated to withstand repeated impacts and return to a complete upright position with minimal maintenance to the unit.
3. **CONSTRUCTION METHODS**
4. **Maintain and Control Traffic.** See Traffic Control Plan.
5. **Staking.** See the Special Note for Staking.
6. **Site Preparation.** Be responsible for all site preparation recommended by the manufacturer or as directed by the Engineer.
7. **Pexco City Post Embedded Anchor Cup.** Install the tubular markerd according to the manufacturer’s recommendations at the location(s) and spacing indicated on the Detail Sheets found elsewhere in the Proposal.

1. **Property Damage.** The Contractor shall be responsible for all damage to public and/or private property resulting from the Contractor’s activities. Repair or replace damaged roadway features in like kind materials and design as directed by the Engineer at no additional cost to the Department. Repair or replace damaged private property in like kind materials and design to the satisfaction of the owner and the Engineer at no additional cost to the Department.
2. **Caution.** The information in this proposal and the type of work listed herein are approximate only and are not to be taken as an exact evaluation of the materials and conditions to be encountered during construction; the bidder must draw his/her own conclusions when developing the Unit Bid Prices for each bid item. As such, if the conditions encountered are not in accordance with the information shown, the Department does not guarantee any changes to the Unit Bid Prices nor extension of the contract will be considered. The Department will pay for bid item quantity overruns, but only if pre-approved by the Engineer.
3. **METHOD OF MEASUREMENT**
4. **Maintain and Control Traffic.** See Traffic Control Plan.
5. **Staking.** See the Special Note for Staking.
6. **Site Preparation.** Other than the bid items listed, the Department will NOT measure Site Preparation for payment, but shall be incidental to the project bid items.
7. **Tubular Markers.** The Department will measure Pexco City Post Embedded Anchor Cup as EACH.
8. **BASIS OF PAYMENT**
9. **Maintain and Control Traffic.** See Traffic Control Plan.
10. **Staking.** See the Special Note for Staking.
11. **Tubular Markers.** The Department will make payment for the completed and accepted quantities under the bid item Tubular Markers (Pexco City Post Embedded Anchor Cup). Payment at the Contract unit price of EACH shall be full compensation for furnishing all materials, equipment, tools, hardware, labor, and incidentals necessary to properly install the Pexco City Post Embedded Anchor Cup according to the manufacturer’s installation instructions, these notes, and/or as directed by the Engineer.